Update to 3.0.21
(from 3.0.18)

On our own behalf:
There are also Mac OS X (10.8.x, 10.9.x, 10.10.x and 10.11.x) and Linux (Ubuntu 12.04 LTS/14.04 LTS, Oracle 6.5 and generic *.tgz) versions  of the UTN Manager available and downloadable at http://www.seh-technology.com/services/downloads.html

Update Note:
"Administrator privileges required for installation"

Important Note:
For all fixes and improvements to work properly with your myUTN devices at least the following firmware/software combination is required:

myUTN-80(HW 1.0):
-----------------
b-fw-ps-22.bin / b-sw-uds-14.3.3.bin

myUTN-50a/250/800 and myUTN-80(HW 2.0):
---------------------------------------
r-fw-uds-14.bin / r-sw-uds-14.4.3.bin

myUTN-55:
---------
r-fw-wlan-5.bin / r-sw-uds-14.4.3.bin

The current myUTN Software can be downloaded from http://www.seh-technology.com/services/downloads.html


General Changes:
################
• Contains several bugfixes and enhancements.
• SEH UTN Manager is now signed with a SHA-256 certificate (valid until 06 April 2018).
	- Microsoft Windows 7 accepts the certificate only if Hotfix KB3033929 (https://support.microsoft.com/en-us/kb/3033929). is installed. You will need Hotfix KB2921916 (https://support.microsoft.com/en-us/kb/2921916) if you want to avoid the „Untrusted Publishers“ dialog for good.
	- A silent installation in Microsoft Windows 7 is not possible.
• Improved compatibility with USB devices.
	- Set up Print-On-Demand might not work after updating to SEH UTN Manager 3.0.21. Solution can be found in SEH Knowledge Base article 50.2.0006 (http://www.seh-technology.com/fileadmin/user/KnowledgeBase/Knowledgebase_0006_en.pdf).

Fixes/Improvements:
###################
• Fixed: CryptoMate64 dongles sometimes caused BSOD if the client system entered energy saving mode (sleep/hibernate)
• Fixed: Simultaneous activation several SafeNet Sentinel Super Pro dongles sometimes caused BSOD
• Fixed: Reconnect of USB devices after network interruptions did not work reliably
• When updating the USB device software an automatic reconnect can be forced by setting a registry value:
	- if you set the registry value (DWORD)
HKLM/SOFTWARE/Wow6432Node/SEH Computertechnik GmbH/SEH UTN Service/reconnectAfterDeinstall 
to 1 (default = 0), the automatic reconnect is activated.
with the registry value (DWORD)
HKLM/SOFTWARE/Wow6432Node/SEH Computertechnik GmbH/SEH UTN Service/reconnectPause 
you can delay the reconnect until the driver installation is finished (default = 20 sec.). The is necessary as the driver installation takes some time and the USB device must not be activated before the installation is finishes. The actual delay is always longer as the configured value because the reactivation list of the SEH UTN Manager is only processed every 10 seconds.
	- Port keys can now be saved in encrypted form, if needed: activate the encryption by setting
HKLM/SOFTWARE/Wow6432Node/SEH Computertechnik GmbH/SEH UTN Manager/options/storePortKeysEnc 
to true (default = false).
Consider encryption carefully: The password created for encryption uses the MAC address of the client.
This may cause problems, e.g. when the client has two network connectors or the network connector is exchanged. In those cases it might be necessary to re-enter the port keys.
If you clone a virtual machine, the MAC address might change and the cloned SEH UTN Manager cannot decrypt the port keys.


Visit the SEH Computertechnik GmbH Homepage (http://www.seh-technology.com) to learn more about Products, Update information, tips, hints & more...