Update to 3.2.10
(from 3.2.7) 

On our own behalf:
OS X/macOS and Linux versions of the SEH UTN Manager are also available at www.seh-technology.com  

Update Note:
Administrator privileges are required for installation.
The new SEH UTN Manager can also be downloaded manually from www.seh-technology.com

Important:
If you install the new SEH UTN Manager, your devices require at least the following firmware/software combination: 

myUTN-2500/INU-100: 
-------------------
p-fw-uds-14.bin / p-sw-uds-14.5.27.bin 	

myUTN-50a/250/800 and myUTN-80(HW 2.0): 
----------------------------------------	
r-fw-uds-19.bin / r-sw-uds-14.5.29.bin 
	
myUTN-55 (HW 1.0): 
------------------
r-fw-wlan-5.bin / r-sw-uds-14.5.29.bin 

myUTN-55 (HW 1.1): 
------------------
r-fw-wlan-12.bin / r-sw-uds-14.5.26.bin

dongleserver Pro / dongleserver ProMAX:
---------------------------------------
p-sys-uds-20.0.21.bin 

utnserver Pro:
---------------------
p-sys-uds-20.0.14.bin 


The current myUTN Software can be downloaded from the SEH Computertechnik GmbH Homepage 
(http://www.seh-technology.com/services/downloads.html).  

General Changes:
################
• Changed the US support number from +1-610-943-3226 to +1-610-933-2088
• Memory leaks (for encrypted connections) closed.
• Continuous improvement of the SEH UTN protocol
• Contains important internal fixes and improvements:

Fixes/Improvements:
###################
•　Rerverse DNS lookup (IP address -> name) disabled. Repeatedly led to problems when it did not match the forward resolution.
• Menu shortcuts (e.g. 'del') now also work directly after program start, even if the corresponding menu has not yet been opened.
•　Fixes and workarounds for the Neural Network Controller V3 (NNCv3 Dongle)

New Devices:
############


Visit the  SEH Computertechnik GmbH Homepage at www.seh-technology.com to learn more about Products, Update information, tips, hints & more...