  ------------------------------!ATTENTION!----------------------------------
ATTENTION!ATTENTION!ATTENTION!ATTENTION!ATTENTION!ATTENTION!ATTENTION!ATTENTION
  ------------------------------!ATTENTION!----------------------------------


PRECONDITION: UTN Manager version 4.x.y

Using this software release on your product requires the most recent UTN Manager version 4.x.y to be installed on any PC that wants to connect with your deviceserver. 

!!The most recent UTN Manager version is NOT provided with this download package!!

Please proceed to the following link and download the most recent UTN Manager: 

http://www.seh-technology.com/services/downloads.html

The software is delivered as it is. SEH Computertechnik GmbH will 
not accept any liability for any error or omission.

If you need further assistance or are unsure which software to use, please 
contact our support team.

Support Contacts & Information:

WEB:   http://www.seh-technology.com/services/support.html
Email: support@seh.de
Phone: +49 (0)521 94226-44                                                                               

----------------------------------------------------------------------------

Binary file: "p-sys-uds-20.2.8.bin"
Version:     20.2.8
Type:        Software for Marvell 381 based deviceserver 
Target:      utnserver Pro HW 3.x
			 utnserver ProMAX
			 dongleserver Pro
             dongleserver ProMAX          
             INU-100 HW 2.x
md5sum:		 74e58985368870931f7a9841f61bc306
sha256sum: 	 61936bc0218dd7d7498f7b2ecdea6e2daf550f372107edab29861a9fc73cbf44

Checksum Info:
The checksum allows to check whether the update file is the file provided by SEH before installation. 

A check can simply be done with e.g. the „shasum“ under macOS/Linux, „sha256sum“ under Linux or under Windows with the „ certutil“ tool, or in Powershell with the "Get-FileHash“ tool. The comparison can then be done manually (the hash values differ dramatically with a slight change) or with the -c option of the checksum commands in one step (see the following example for macOS/Linux):

Example macOS/Linux:
shasum -a 256 [FILENAME]

➔ echo '61936bc0218dd7d7498f7b2ecdea6e2daf550f372107edab29861a9fc73cbf44 *p-sys-uds-20.2.8.bin' | shasum -c
p-sys-uds-20.2.8.bin: OK


Example Windows:
Windows command prompt:
CertUtil -hashfile [FILENAME] SHA256
C:>certutil -hashfile p-sys-uds-20.2.8.bin SHA256
SHA256 hash of p-sys-uds-20.2.8.bin:
61936bc0218dd7d7498f7b2ecdea6e2daf550f372107edab29861a9fc73cbf44
CertUtil: -hashfile command completed successfully.

Release Notes:
---------------------------------------------------------------------------
New Software Version:   			20.2.8
New Features/Changes/Fixes: since 	20.2.6

Important Upgrade Note:
#######################
Important Upgrade Note:
#######################
Backup your current settings before upgrading.
Only a parameter backup ensures all configurations are preserved if you need to downgrade. 

1) General:
-----------
- OpenSSL LTS Version 3.5.4
- Contains  fixes and improvements
- Backend improvements for enhanced stability, device compatibility, and protocol handling.
 
 2) Fixes/Improvements:
----------------------
- [Improved] HID/MSD detection is now visually indicated in the Control Center. The corresponding checkboxes are highlighted with a border if a connected USB device is detected as a Human Interface Device (HID) or Mass Storage Device (MSD).
- [Fixed] HID/MSD blocking settings now take effect immediately after saving and no longer require a restart of the UTN server.
- [Fixed] USB port information is now included for all recipients of USB device status change notifications. Previously, only the first email recipient received the detailed USB port information.
- [Improved] The Control Center security warning has been updated for devices upgraded from an earlier software version. If existing passwords do not meet the current password requirements, the warning now clearly indicates that the passwords must be updated. This helps clarify cases where passwords are already set but no longer comply with the current security policy.
- [Fixed] The Control Center now displays an error message when saving a USB Manager password that does not meet the current password requirements. Previously, the change was reported as successful although the password was not accepted and the parameter remained unchanged.
- [Fixed] [dongleserver ProMAX/INU-100] Access protection for sensitive files stored on the SD card has been improved. Previously, after removing and reinserting the SD card, certain sensitive files could become accessible via the internal file browser to an authenticated administrator. These files are now protected as intended.
- [Fixed] [INU-50] Resolved an issue where devices could only be activated once. A second activation could cause the device to repeatedly switch between activated and deactivated states.

3) New Devices:
---------------
-  Feitian Technologies, Inc. Dongles with Feitian ePass OTP Tool
(https://www.ftsafe.com/Products)

SOFTWARE DOWNLOAD
---------------------------------------------------------------------------
New software/firmware versions can be downloaded to your product via
network file transfer. The following text describes a download using
the SEH Product Manager and HTTP.

Note: We recommend unencrypted HTTP instead of HTTPs.

1) HTML (HTTP-protocol)
------------------------
Start a web browser and type in the IP address of your product. Proceed to the 
Control Center of your product. Choose "MAINTENANCE" in the left menu. 
Select "Update" in the left menu. Select the file and press the INSTALL button.

Note: Depending on the network throughput the download may take several seconds.
Please be patient.

2) SEH Product Manager
------------------------
Start the SEH Product Manager and select your product.

Right-click your product in the device list.
Select 'Load software .. from the shortcut menu. Select the
file. Click 'OK' and confirm the selection. Once the file has
been downloaded the product restarts automatically.

Note: Depending on the network throughput the download may take several
      seconds. Please be patient.


-------------------------------------------------------------------------------
Visit the  SEH Computertechnik GmbH Homepage at www.seh-technology.com to learn more about Products, Update information, tips, hints & more...